help
Manage aliases kept in FLASH memory
   alias name [value]
Set/Query the system console baud rate
   baudrate [-b <rate>]
Manage machine caches
   cache [ON | OFF]
Execute an image
   exec [-b <argv addr>] [-c "kernel command line"] [-w <timeout>]
        [<entry point>]
Manage FLASH images
   fis {cmds}
Manage configuration kept in FLASH memory
   fconfig [-i] [-l] [-n] [-f] [-d] | [-d] nickname [value]
Help about help?
   help [<topic>]
Display command history
   history 
Set/change IP addresses
   ip_address [-l <local_ip_address>[/<mask_len>]] [-h <server_address>]
Load a file
   load [-r] [-v] [-d] [-h <host>] [-p <TCP port>][-m <varies>] [-c <channel_number>] 
        [-b <base_address>] <file_name>
Reset the system
   reset 
Display RedBoot version information
   version 
DD-WRT> 